Safety and Work Protocol for RC2 Woollam Ellipsometer:
Only Trained and Authorized Users are Allowed to Operate the System !
· Use gloves when handling with the system to prevent contamination.
· Power on the ellipsometer in the following order: power unit, light source unit, and then the software (the computer password is” Woollam!”).
· Ensure that your sample is clean; otherwise, it may affect the measurements.
· Select an appropriate recipe for your sample; you are not allowed to modify any existing recipes in the software.
· The system software is intended for brief analyses. For in-depth analyses, a separate computer is available for remote connection.
· If a malfunction occurs, immediately stop work, report the issue to the tool owner.
· Power off the ellipsometer in the following order: light source unit, software, computer and then the power unit.
Additional Accessories
To use the temperature-controlled stage or focusing probes, please coordinate with the tool owner.

For any questions, call 79812/ 08-6479812 Tania
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